LED escape sign luminaire in accordance with DIN EN 60598-1, DIN EN 60598-2-22, DIN EN 7010 and DIN EN 1838Plastic disc escape sign luminaire for surface mounting on walls and for marking escape and rescue routes. Levelling screws are integrated to facilitate installation and compensate for uneven surfaces. Planning reliability is ensured by the tool-free, variable use of the pictograms on site. The pictograms are inserted solvent-free. The pictogram set (top, bottom, right and left arrows) is included as standard.

Monitoring: 
With integrated monitoring module, for operation on a 24V power supply system. Automatic test system in accordance with DIN EN 62034 type ER, in conjunction with a CoreCompact system. Functions must be complied with:
· Integrated individual luminaire monitoring
· Automatic addressing via configuration wizard
· Luminaires can be individually programmed and dimmed with RP's central power supply system
· Luminaire update via the system
Material: Polycarbonate
Color: RAL 9003
Dimensions: 56.1 mm x 417.5 mm x 245.5 mm

Mounting method: Wandaufbau
Protection class: 2
Protection rating (IP): IP 40
Impact restistence rate IK: IK 5
Allowed temperature DS: -5 °C to 40 °C °C
Allowed temperature BS: -5 °C to 40 °C °C
Viewing distance: 40m m
Pictogram: Einzeln n.A.

Power maintained mode: 3,7 W W
Power non-maintained mode: 0,4 W W

Input voltage AC: 24 V V
Connection terminals: 2.5 mm² mm

Battery: 

Article number: GABW509CC

Accessories:

Brand: RP-Technik GmbH
