Emergency sign / safety light in accordance to DIN EN 60598-1, DIN EN 60598-2-22 and DIN EN 1838.   Slim, convex, synthetic luminaire for wall mounting. Emergency sign luminaire with pluggable, solvent-free, internal set of pictograms (left, right, bottom, top) included in the scope of delivery. Also usable as safety light without applying the pictograms, as it includes a clear-transparent cover. Evenly distributed illumination, due to the alligned and chromed reflector. Suitable for continuous mode or stand-by mode. 

Monitoring: 
With integrated monitoring module for operating on a Wireless Professional central monitoring system.
· Charge monitoring indicator on the luminaire
· Manual or automatic function test (free choice of test start time in the WirelessControl software)
· Manual or automatic continuous function test can be activated via the length of the luminaire’s measurement operation (free choice of test start times in the WirelessControl software)
· Automatic charge monitoring
· Deep discharge protection with restart inhibit
Material: Polycarbonate
Color: RAL 9003
Dimensions: 170 mm x 340 mm x 60 mm

Mounting method: Universal
Protection class: 2
Protection rating (IP): IP 54
Impact restistence rate IK: IK 6
Allowed temperature DS: -5 °C to 40 °C °C
Allowed temperature BS: -5 °C to 40 °C °C
Pictogram: Nein

Power maintained mode: 5,7 W W
Power non-maintained mode: 0,8 W W
Luminous Flux Emergency Operation: 520 lm lm

Input voltage AC: 230 V V
Connection terminals: 2.5 mm² mm

Battery: LFPN3233.01-SET

Article number: KCW423WL

Accessories:
Article number: BALL2, Ball protection (8W) 450x280x125mm  RAL9010, for KCW, KL, LX, VX, PFW
Article number: DWKCW, ceiling bracket KC wall
Article number: KC-IP65, KC gasket IP65 EPDM
Article number: KCER, KCW recessed frame
Article number: KCWFH, flexible wall mounting for KCW
Article number: LSYS-B4, 4x Beam lens for lights with a lens system, for  example for lighting first aid or fire alarm  systems
Article number: LSYS-F4, 4x corridor lenses for luminaires with lens  system
Article number: LSYS-H4, 4x h-lenses for luminaires with lens  system
Article number: LSYS-R4, 4x  round lenses for luminaires with lens  system
Article number: LSYS-S4, 4x Spotlens for luminares with lens system.  Suitable for ceilings up to 12m
Article number: LSYS-WF4, 4x wall corridor lenses for luminaires with lens  system
Article number: LFP3233-SET-2AKKU

Brand: RP-Technik GmbH
