The CBU TED module is an elegant Bluetooth-controlled trailing edge dimmer from CASAMBI®, which enables continuous dimming for all available illuminants. It can be installed both behind a conventional wall switch or directly in a luminaire or a terminal box. With the new long-range feature, you can now also enjoy reliable control from even greater distances.

Electrical connection:
Power maintained: 100 W
Input voltage AC: 220-240V / 50-60Hz V

label.zuordnungsspeicher.gruppe.Casambi-Products:
Max. transmission power: +4 dBm

Brand: RP-Technik GmbH
