Escape Route Luminaire with ERT LED for Trilux E-Line Trunking System (Profile 07650, 7-core)This escape route luminaire is specifically designed for the Trilux E-Line trunking system with a 7-core profile (07650). The integrated, innovative lens holder with quick-mounting functionality allows for easy and flexible use of different lens types – perfectly tailored to the specific application.The scope of delivery includes both a lens for area lighting and one for corridor lighting.

Monitoring: 
Version with automatic test system in accordance with DIN EN 62034 type S including SelfControl test button:
· Test results with fault analysis (illuminant, charge and battery circuit) and status displays (operation, function test, continuous function test) using 3 colour LEDs
· Automatic function test (weekly)
· Automatic continuous function test (every 12 months)
· Automatic charge monitoring
· Deep discharge protection with restart inhibit
· Idling and short-circuit shutdown of inverter
Material: Metal
Color: RAL 9003
Dimensions: 368 mm x 62 mm x 40.7 mm

Mounting method: Schienensysteme
Protection class: 1
Protection rating (IP): IP 20
Impact restistence rate IK: IK 3
Allowed temperature DS: -5 °C to 40 °C °C
Allowed temperature BS: -5 °C to 40 °C °C
Pictogram: Nein

Power maintained mode: 5,6 W W
Power non-maintained mode: 2 W W
Luminous Flux Emergency Operation: 470 lm lm

Input voltage AC: 250 V V
Connection terminals: 2,5 mm² mm

Battery: LFPN3212.01-SET

Article number: LBLT431SC

Accessories:

Brand: RP-Technik GmbH
