
Monitoring: 
With integrated monitoring module with 20-digit addressing switch, for operation on a central power supply system. Automatic test system according to DIN EN 62034 type ER, in connection with a system of type MultiControl. Functions must be complied with:
· Integrated individual luminaire monitoring
· Integrated luminaire manager function
· Individual switchability in conjunction with RP ELS - central power supply system
Material: Zinc die-cast
Color: RAL 7016
Diameter: 160 mm

Mounting method: Bodenaufbau
Protection class: 1
Protection rating (IP): IP 65
Impact restistence rate IK: IK 10
Allowed temperature DS: -20 °C to 50 °C °C
Allowed temperature BS: -20 °C to 50 °C °C
Pictogram: Nein

Power maintained mode: 11,5 W W
Power non-maintained mode: 1,5 W W
Luminous Flux Emergency Operation: 610 lm lm

Input voltage AC: 230 V V

Battery: 

Article number: ZPMR029ML

Accessories:

Brand: RP-Technik GmbH
