LED diffuser light "VASCA"LED diffuser light, VASCA series, IP66, IK08. Polycarbonate housing. Prismatic diffuser made of PC, UV-resistant. Diffuser fastened with stainless steel clips. LED circuit board individually replaceable. Built-in DALI Power-driver. Through-Wiring available. DC compatible. The power (20-36W) and the colour temperature (3000-4000-5000K) can be set via dip switch.

Dimensions:
Width: 99 mm
Height: 82 mm
Depth: 1268 mm

Packaging dimensions:
Width: 104 mm
Height: 84 mm
Depth: 1270 mm

Cutout Dimensions:

Color:

Housing material:

Certification:
Protection type (IP): wert.IngressProtection.IP 66
Shock resistance level (IK): wert.IKclass.IK 8

Storage temperature range:

Housing temperature tc (Max):

Electrical connection:

power supply:
DC suitability: wert.DCSuitable.Ja

Light data:
Light source: wert.LightSource.LED
Rated luminous flux: 2880-5040 lm
Color temperature: 3000/4000/5000 K
UGR: 24

Temperatures:

Mounting:

Brand: RP-Technik GmbH
