Emergency sign luminaire in accordance with DIN EN 60598-1, DIN EN 60598-2-22 and DIN EN 1838.   Slim, elegant, convex plastic luminaire inclined towards the viewer, tapering symmetrically downwards. For universal mounting (wall/ceiling). Suitable for continuous or standby operation. Planning reliability thanks to tool-free, variable use of pictograms on site. The pictograms comply with DIN ISO 7010 (2x man in door and two arrows) and are  inserted internally and are solvent-free. 

Monitoring: 
With integrated monitoring module with 20-digit addressing switch, for operation on a central power supply system. Automatic test system according to DIN EN 62034 type ER, in connection with a system of type MultiControl. Functions must be complied with:
· Integrated individual luminaire monitoring
· Integrated luminaire manager function
· Individual switchability in conjunction with RP ELS - central power supply system
Material: Polycarbonate
Color: RAL 9003
Dimensions: 212 mm x 31 mm x 141 mm

Mounting method: Universal
Protection class: 2
Protection rating (IP): IP 40
Impact restistence rate IK: IK 5
Allowed temperature DS: -20 °C to 40 °C °C
Allowed temperature BS: -20 °C to 40 °C °C
Viewing distance: 20m m
Pictogram: Set

Power maintained mode: 2,7 W W
Power non-maintained mode: 0,9 W W

Input voltage AC: 230 V V
Connection terminals: 2,5 mm² mm

Battery: 

Article number: KFMU009ML

Accessories:

Brand: RP-Technik GmbH
