Emergency sign luminaire in accordance with DIN EN 60598-1, DIN EN 60598-2-22 and DIN EN 1838.   Slim, elegant, convex plastic luminaire inclined towards the viewer, tapering symmetrically downwards. For universal mounting (wall/ceiling). Suitable for continuous or standby operation. Planning reliability thanks to tool-free, variable use of pictograms on site. The pictograms comply with DIN ISO 7010 (2x man in door and two arrows) and are  inserted internally and are solvent-free. 
Monitoring: 
With integrated monitoring module, for operation on a 24V power supply system. Automatic test system in accordance with DIN EN 62034 type ER, in conjunction with a CoreCompact system. Functions must be complied with:
· Integrated individual luminaire monitoring
· Automatic addressing via configuration wizard
· Luminaires can be individually programmed and dimmed with RP's central power supply system
· Luminaire update via the system
Material: Polycarbonate
Color: RAL 9003
Dimensions: 212 mm x 31 mm x 141 mm

Mounting method: Universal
Protection class: 3
Protection rating (IP): IP 40
Impact restistence rate IK: IK 5
Allowed temperature DS: -30 °C to 40 °C °C
Allowed temperature BS: -30 °C to 40 °C °C
Viewing distance: 20m m
Pictogram: Set

Power maintained mode: 2,00 W W
Power non-maintained mode: 0,4 W W

Battery: 

Article number: KFMU509CC

Accessories:

Brand: RP-Technik GmbH
