Die-cast zinc disc light in accordance with DIN EN60598-1, DIN EN 60598-2-22 and DIN EN 1838.German Design Award 2018 winner: zinc die-cast LED disc light for wall mounting. The simple and clear design language of all A-series light variants allows them to be integrated into any type of building. The modular, practical design of the A-series promises easy installation for all variants. The design is perfectly adapted to any type of installation. Features:- Mechanically robust and corrosion-resistant- Powder-coated surface- Precise edges and straight lines- No weld seams or bent edges- Solvent-free attachment of pictogram- Disc with polished edges and continuous, invisible pictogram holder- Mounting housing identical for all A-series variants.Suitable for permanent or standby switching. Planning reliability thanks to tool-free, variable use of pictograms on site. Pictograms in accordance with DIN EN ISO 7010 and DIN ISO 3864 (left, right, bottom, top) included as standard.  

Monitoring: 
Version with automatic test system in accordance with DIN EN 62034 type S including SelfControl test button:
· Test results with fault analysis (illuminant, charge and battery circuit) and status displays (operation, function test, continuous function test) using 3 colour LEDs
· Automatic function test (weekly)
· Automatic continuous function test (every 12 months)
· Automatic charge monitoring
· Deep discharge protection with restart inhibit
· Idling and short-circuit shutdown of inverter
Material: Zinc die-cast
Color: RAL 7016
Dimensions: 55 mm x 193 mm x 120 mm

Mounting method: Wandaufbau
Protection class: 2
Protection rating (IP): IP 40
Impact restistence rate IK: IK ≥ 3
Allowed temperature DS: -5 °C to 40 °C °C
Allowed temperature BS: -5 °C to 40 °C °C
Viewing distance: 15m m
Pictogram: Set

Power maintained mode: 2,6 W W
Power non-maintained mode: 0,9 W W

Input voltage AC: 250 V V

Battery: LFPN3212.01-SET

Article number: AIW401SC-AZ

Accessories:

Brand: RP-Technik GmbH
