Die-cast zinc disc light in accordance with DIN EN60598-1, DIN EN 60598-2-22 and DIN EN 1838.German Design Award 2018 winner: zinc die-cast LED disc light for wall mounting. The simple and clear design language of all A-series light variants allows them to be integrated into any type of building. The modular, practical design of the A-series promises easy installation for all variants. The design is perfectly adapted to any type of installation. Features:- Mechanically robust and corrosion-resistant- Powder-coated surface- Precise edges and straight lines- No weld seams or bent edges- Solvent-free attachment of pictogram- Disc with polished edges and continuous, invisible pictogram holder- Mounting housing identical for all A-series variants.Suitable for permanent or standby switching. Planning reliability thanks to tool-free, variable use of pictograms on site. Pictograms in accordance with DIN EN ISO 7010 and DIN ISO 3864 (left, right, bottom, top) included as standard.  

Monitoring: 
With integrated monitoring module, for operation on a 24V power supply system. Automatic test system in accordance with DIN EN 62034 type ER, in conjunction with a CoreCompact system. Functions must be complied with:
· Integrated individual luminaire monitoring
· Automatic addressing via configuration wizard
· Luminaires can be individually programmed and dimmed with RP's central power supply system
· Luminaire update via the system
Material: Zinc die-cast
Color: RAL 9003
Dimensions: 55 mm x 193 mm x 120 mm

Mounting method: Wandaufbau
Protection class: 2
Protection rating (IP): IP 40
Impact restistence rate IK: IK ≥ 3
Allowed temperature DS: -5 °C to 40 °C °C
Allowed temperature BS: -5 °C to 40 °C °C
Viewing distance: 15m m
Pictogram: Set

Power maintained mode: 1,7 W W
Power non-maintained mode: 0,4 W W

Input voltage AC: 24 V V
Connection terminals: 2.5 mm² mm

Battery: 

Article number: AIW509CC

Accessories:

Brand: RP-Technik GmbH
