Emergency sign luminaire in accordance with DIN EN 60598-1, DIN EN 60598-2-22 and DIN EN 1838Plastic LED emergency sign luminaire with convex cover for wall mounting. Suitable for continuous or standby operation. Levelling screws are integrated to compensate for uneven surfaces and facilitate installation. Planning reliability is ensured by the tool-free, variable use of pictograms on site. The pictograms are internal and are inserted without the use of solvents. The pictogram set (MTL, MTR and 2x straight arrow) is included as standard.

Monitoring: 
Version with automatic test system in accordance with DIN EN 62034 type S including SelfControl test button:
· Test results with fault analysis (illuminant, charge and battery circuit) and status displays (operation, function test, continuous function test) using 3 colour LEDs
· Automatic function test (weekly)
· Automatic continuous function test (every 12 months)
· Automatic charge monitoring
· Deep discharge protection with restart inhibit
· Idling and short-circuit shutdown of inverter
Material: Polycarbonate
Color: RAL 9003
Dimensions: 65 mm x 236 mm x 136 mm

Mounting method: Wandaufbau
Protection class: 2
Protection rating (IP): IP 65
Impact restistence rate IK: IK 6
Allowed temperature DS: -15 °C to 40 °C °C
Allowed temperature BS: -15 °C to 40 °C °C
Viewing distance: 20m m
Pictogram: Set

Power maintained mode: 4 W W
Power non-maintained mode: 2 W W

Input voltage AC: 250 V V
Connection terminals: 2,5 mm² mm

Battery: LFPN3233.01-TT-SET

Article number: PMW408SC-TT

Accessories:
Article number: PME, Recessed frame ABS white for PMD and PMW  luminaires
Article number: LFPN3233.01-TT

Brand: RP-Technik GmbH
