General and emergency lighting in accordance with DIN EN 60598-1, DIN EN 60598-2-22 and DIN EN 1838Elegant, round LED general light fitting made of aluminium for wall or ceiling mounting with emergency light insert.  Choice of aluminium anodised or white housing colourChoice of 4000 K or 3000 K light colour

Monitoring: 
With integrated monitoring module, for operation on a 24V power supply system. Automatic test system in accordance with DIN EN 62034 type ER, in conjunction with a CoreCompact system. Functions must be complied with:
· Integrated individual luminaire monitoring
· Automatic addressing via configuration wizard
· Luminaires can be individually programmed and dimmed with RP's central power supply system
· Luminaire update via the system
Material: Aluminum
Color: RAL 9003
Diameter: 395 mm

Mounting method: Universal
Protection class: 1
Protection rating (IP): IP 20
Impact restistence rate IK: IK ≥ 3
Allowed temperature DS: -20 °C to 30 °C °C
Allowed temperature BS: -20 °C to 40 °C °C
Pictogram: Nein

Power maintained mode: 2,8 W W
Power non-maintained mode: 0,4 W W
Luminous Flux Emergency Operation: 240 lm lm

Input voltage AC: 24 V V
Connection terminals: 2.5 mm² mm

Battery: 

Article number: QAW529CC

Accessories:

Brand: RP-Technik GmbH
