LED escape sign luminaire for wall mounting in accordance with DIN EN 60598-1, DIN EN 60598-2-22 and DIN EN 1838.Wall-mounted escape sign luminaire in square format with frameless cover and easy-to-install bayonet catchSuitable for permanent or standby switching.Includes pictogram in accordance with DIN EN ISO 7010 and DIN ISO 3864 (left, right, top or bottom). Optionally, the luminaire can be used for labelling other side rooms.

Monitoring: 
With integrated monitoring module for operating on a Wireless Professional central monitoring system.
· Charge monitoring indicator on the luminaire
· Manual or automatic function test (free choice of test start time in the WirelessControl software)
· Manual or automatic continuous function test can be activated via the length of the luminaire’s measurement operation (free choice of test start times in the WirelessControl software)
· Automatic charge monitoring
· Deep discharge protection with restart inhibit
Material: Polycarbonate
Color: RAL 9003
Dimensions: 400 mm x 400 mm x 110 mm

Mounting method: Wandaufbau
Protection class: 2
Protection rating (IP): IP 65
Impact restistence rate IK: IK 4
Allowed temperature DS: -15 °C to 40 °C °C
Allowed temperature BS: -15 °C to 40 °C °C
Viewing distance: 40m m
Pictogram: Einzeln n.A.

Power maintained mode: 5,7 W W
Power non-maintained mode: 0,8 W W
Luminous Flux Emergency Operation: 520 lm lm

Input voltage AC: 230 V V
Connection terminals: 2.5 mm² mm

Battery: LFPN3233.01-TT-SET

Article number: WFBW413WL-TT

Accessories:
Article number: LFP3233.01-TT-SET-2AKKUS, LiFePO4 3,2V /  3,3Ah, low temperature

Brand: RP-Technik GmbH
