General and emergency lighting in accordance with DIN EN 60598-1, DIN EN 60598-2-22 and DIN EN 1838Elegant, round LED general light fitting made of aluminium for wall or ceiling mounting with emergency light insert. Emergency lighting is provided by an additional integrated emergency light.  Choice of aluminium anodised or white housing colourChoice of 4000K light colour with luminous flux in mains operation 2300 lm or 3000K

Monitoring: 
With integrated monitoring module for operation on a monitoring device of the Wireless Basic type.
· Time-saving configuration and commissioning as well as monitoring via Bluetooth using an Android app
· Operation in offline mode or optionally via LIGHTLINX® with versatile cloud functions
· Version with automatic test system according to DIN EN 62034 type S incl. SelfControl test button
· Test results with fault analysis (illuminant, charging and battery circuit) as well as status displays (operation, function test, duration test) via 3 coloured LEDs
· Manual or automatic function test (test start time freely selectable in the WirelessBasic app)
· Configurable duration test (every 12 months)
· Automatic charge monitoring
· Deep discharge protection with restart lockout
· No-load and short-circuit shutdown of the inverter
Material: Aluminum
Color: Alu eloxiert
Diameter: 395 mm

Mounting method: Universal
Protection class: 1
Protection rating (IP): IP 20
Impact restistence rate IK: IK ≥ 3
Allowed temperature DS: -5 °C to 30 °C °C
Allowed temperature BS: -5 °C to 35 °C °C
Pictogram: Nein

Power maintained mode: 26,4 W W
Power non-maintained mode: 0,4 W W
Luminous Flux Emergency Operation: 125 lm lm

Input voltage AC: 230 V V
Connection terminals: 2.5 mm² mm

Battery: LFPN3233.01, {{Produkt - BatteryPerformance - BatteryTechnology (P:17:110)}} Battery

Article number: QAW428WB-SIWW

Accessories:

Brand: RP-Technik GmbH
