
Monitoring: 
With integrated monitoring module with 20-digit addressing switch, for operation on a central power supply system. Automatic test system according to DIN EN 62034 type ER, in connection with a system of type MultiControl. Functions must be complied with:
· Integrated individual luminaire monitoring
· Integrated luminaire manager function
· Individual switchability in conjunction with RP ELS - central power supply system
Material: PCABS,Polycarbonate
Color: RAL 9003
Dimensions: 73 mm x 339 mm x 71 mm

Mounting method: Deckenaufbau
Protection class: 2
Protection rating (IP): IP 65
Impact restistence rate IK: IK 8
Allowed temperature DS: -20 °C to 50 °C °C
Allowed temperature BS: -20 °C to 50 °C °C
Pictogram: Nein

Power maintained mode: 5,2 W W
Power non-maintained mode: 1,1 W W
Luminous Flux Emergency Operation: 520 lm lm

Input voltage AC: 230 V V
Connection terminals: 2.5 mm² mm

Battery: 

Article number: PXDL029ML

Accessories:
Article number: PXD-AW, wall-parallel-bracket for the luminaire type  PXD

Brand: RP-Technik GmbH
