
Monitoring: 
Version with automatic test system in accordance with DIN EN 62034 type S including SelfControl test button:
· Test results with fault analysis (illuminant, charge and battery circuit) and status displays (operation, function test, continuous function test) using 3 colour LEDs
· Automatic function test (weekly)
· Automatic continuous function test (every 12 months)
· Automatic charge monitoring
· Deep discharge protection with restart inhibit
· Idling and short-circuit shutdown of inverter
Material: PCABS,Polycarbonate
Color: RAL 9003
Dimensions: 73 mm x 339 mm x 71 mm

Mounting method: Deckenaufbau
Protection class: 2
Protection rating (IP): IP 65
Impact restistence rate IK: IK 8
Allowed temperature DS: 0 °C to 40 °C °C
Allowed temperature BS: 0 °C to 40 °C °C
Pictogram: Nein

Power maintained mode: 5,2 W W
Power non-maintained mode: 0,8 W W
Luminous Flux Emergency Operation: 210 lm lm

Input voltage AC: 250 V V
Connection terminals: 2,5 mm² mm

Battery: LFPN3233.01-SET

Article number: PXDL428SC

Accessories:
Article number: PXD-AW, wall-parallel-bracket for the luminaire type  PXD

Brand: RP-Technik GmbH
