
Monitoring: 
With integrated monitoring module, for operation on a 24V power supply system. Automatic test system in accordance with DIN EN 62034 type ER, in conjunction with a CoreCompact system. Functions must be complied with:
· Integrated individual luminaire monitoring
· Automatic addressing via configuration wizard
· Luminaires can be individually programmed and dimmed with RP's central power supply system
· Luminaire update via the system
Material: PCABS,Polycarbonate
Color: RAL 9003
Dimensions: 73 mm x 339 mm x 71 mm

Mounting method: Deckenaufbau
Protection class: 2
Protection rating (IP): IP 65
Impact restistence rate IK: IK 8
Allowed temperature DS: -20 °C to 50 °C °C
Allowed temperature BS: -20 °C to 50 °C °C
Pictogram: Nein

Power maintained mode: 5,1 W W
Power non-maintained mode: 0,4 W W
Luminous Flux Emergency Operation: 520 lm lm

Input voltage AC: 24 V V
Connection terminals: 2.5 mm² mm

Battery: 

Article number: PXDL529CC

Accessories:
Article number: PXD-AW, wall-parallel-bracket for the luminaire type  PXD

Brand: RP-Technik GmbH
