Die-cast zinc disc light in accordance with DIN EN60598-1, DIN EN 60598-2-22 and DIN EN 1838.German Design Award 2018 winner: die-cast zinc LED disc light for surface-mounted ceiling installation with pendant suspension. Sober and clear design language of all A-series luminaire variants for integration into any type of building. The modular, practical design of the A-series promises the simplest installation for all variants. The design is perfectly matched for any type of installation. Features:- Mechanically robust and corrosion-resistant- Powder-coated surface- Precise edges and straight lines- No weld seams or bent edges- Square suspension rod 125 mm, can be shortened as required- LED power supply in the suspension- Solvent-free attachment of the pictogram- Disc with polished edges and continuous, invisible pictogram holder- Mounting housing identical for all A-series variantsSuitable for continuous or standby switching. Planning reliability thanks to tool-free, variable use of pictograms on site. Pictograms in accordance with DIN EN ISO 7010 and DIN ISO 3864 (left, right, bottom, top) included as standard.  Translated with DeepL.com (free version)

Monitoring: 
With integrated monitoring module with 20-digit addressing switch, for operation on a central power supply system. Automatic test system according to DIN EN 62034 type ER, in connection with a system of type MultiControl. Functions must be complied with:
· Integrated individual luminaire monitoring
· Integrated luminaire manager function
· Individual switchability in conjunction with RP ELS - central power supply system
Material: Zinc die-cast
Color: RAL 9003
Dimensions: 80 mm x 196 mm x 289 mm

Mounting method: Deckenaufbau-Pendel
Protection class: 2
Protection rating (IP): IP 40
Impact restistence rate IK: IK ≥ 3
Allowed temperature DS: -5 °C to 40 °C °C
Allowed temperature BS: -5 °C to 40 °C °C
Viewing distance: 15m m
Pictogram: Set

Power maintained mode: 2,6 W W
Power non-maintained mode: 1,1 W W

Input voltage AC: 230 V V
Connection terminals: 2.5 mm² mm

Battery: 

Article number: AIDP009ML

Accessories:
Article number: AM-X-PKG

Brand: RP-Technik GmbH
