
Monitoring: 
Integrated monitoring module for operation with a DALI 2 type monitoring device
· Version with automatic test system according to DIN EN 62034; the type depends on the control unit.
· Automatic test results with fault analysis and status display (operation, function test, endurance test) centrally and at the luminaire via three LEDs.
· Manual or automatic function test configurable by group (test start time freely selectable in the DALI software).
· Configurable endurance test (every 12 months).
· Automatic charging monitoring.
· Deep discharge protection with restart lockout.
Material: PCABS,Polycarbonate
Color: RAL 9003
Dimensions: 73 mm x 339 mm x 71 mm

Mounting method: Deckenaufbau
Protection class: 2
Protection rating (IP): IP 65
Impact restistence rate IK: IK 8
Allowed temperature DS: 0 °C to 40 °C °C
Allowed temperature BS: 0 °C to 40 °C °C
Pictogram: Nein

Power maintained mode: 5,2 W W
Power non-maintained mode: 1,0 W W
Luminous Flux Emergency Operation: 520 lm lm


Battery: LFPN3233.01, {{Produkt - BatteryPerformance - BatteryTechnology (P:17:110)}} Battery

Article number: PXDL423DL

Accessories:
Article number: PXD-AW, wall-parallel-bracket for the luminaire type  PXD

Brand: RP-Technik GmbH
