LED safety luminaire according to DIN EN 60598-1, DIN EN 60598-2 and DIN EN 1838Square zinc die-cast luminaire for ceiling mounting. Spring fastening for easy mounting. Optimal light Distribution and lighting of escape and rescue routes is achieved by using diffuser lenses and efficent LED ERT Technology. The result are greatly increased mounting distances. The illuminant is exchangeable and has an integrated Status LED within the lens but only with the single battery variant. Mounting in normal Installation boxes or in fire protection boxes Ø68 mm with an Adapter (EE-EBA).

Monitoring: 
Integrated monitoring module for operation with a DALI 2 type monitoring device
· Version with automatic test system according to DIN EN 62034; the type depends on the control unit.
· Automatic test results with fault analysis and status display (operation, function test, endurance test) centrally and at the luminaire via three LEDs.
· Manual or automatic function test configurable by group (test start time freely selectable in the DALI software).
· Configurable endurance test (every 12 months).
· Automatic charging monitoring.
· Deep discharge protection with restart lockout.
Material: Zinc die-cast
Color: RAL 9003
Diameter: 88 mm

Mounting method: Deckeneinbau
Protection class: 2
Protection rating (IP): IP 20
Impact restistence rate IK: IK ≥ 3
Allowed temperature DS: -5 °C to 40 °C °C
Allowed temperature BS: -5 °C to 40 °C °C
Pictogram: Nein

Power maintained mode: 3,6 W W
Power non-maintained mode: 0,9 W W
Luminous Flux Emergency Operation: 235 lm lm


Battery: LFPN3212.01-SET

Article number: EERL433DL

Accessories:

Brand: RP-Technik GmbH
