Safety light in accordance with DIN EN 60598-1, DIN EN 60598-2-22 and DIN EN 1838Plastic LED emergency light with convex moulded cover for ceiling or wall mounting. Suitable for permanent or standby switching. Levelling screws are integrated to make installation easier and compensate for uneven surfaces.The innovative integrated lens holder with quick-mounting device enables the flexible use of different lens types. The most versatile application in this luminaire is the corridor lens, which is already fitted. If necessary, they can be easily replaced with lenses with the desired beam characteristics. This flexibility makes it easy to adapt to the respective installation situation.

Monitoring: 
Version with automatic test system in accordance with DIN EN 62034 type S including SelfControl test button:
· Test results with fault analysis (illuminant, charge and battery circuit) and status displays (operation, function test, continuous function test) using 3 colour LEDs
· Automatic function test (weekly)
· Automatic continuous function test (every 12 months)
· Automatic charge monitoring
· Deep discharge protection with restart inhibit
· Idling and short-circuit shutdown of inverter
Material: Polycarbonate
Color: RAL 9003
Dimensions: 65 mm x 236 mm x 136 mm

Mounting method: Universal
Protection class: 2
Protection rating (IP): IP 65
Impact restistence rate IK: IK 6
Allowed temperature DS: -5 °C to 40 °C °C
Allowed temperature BS: -5 °C to 40 °C °C
Pictogram: Nein

Power maintained mode: 5,6 W W
Power non-maintained mode: 2 W W
Luminous Flux Emergency Operation: 520 lm lm

Input voltage AC: 250 V V
Connection terminals: 2,5 mm² mm

Battery: LFPN3216.01-SET

Article number: PMW421SC-F-OEM

Accessories:
Article number: LFP3216-SET-2AKKU

Brand: RP-Technik GmbH
