
Monitoring: 
Version with automatic test system in accordance with DIN EN 62034 type S including SelfControl test button:
· Test results with fault analysis (illuminant, charge and battery circuit) and status displays (operation, function test, continuous function test) using 3 colour LEDs
· Automatic function test (weekly)
· Automatic continuous function test (every 12 months)
· Automatic charge monitoring
· Deep discharge protection with restart inhibit
· Idling and short-circuit shutdown of inverter
Material: Zinc die-cast
Color: RAL 7016
Diameter: 160 mm

Mounting method: Bodenaufbau
Protection class: 1
Protection rating (IP): IP 65
Impact restistence rate IK: IK 10
Allowed temperature DS: -20 °C to 50 °C °C
Allowed temperature BS: -20 °C to 50 °C °C
Pictogram: Nein

Power maintained mode: 11,5 W W
Power non-maintained mode: 0,7 W W
Luminous Flux Emergency Operation: 200 lm lm

Input voltage AC: 240 V V
Connection terminals: 1,5 mm² mm

Battery: LFPN3260.WRLEN, {{Produkt - BatteryPerformance - BatteryTechnology (P:17:110)}} Battery

Article number: ZPMR403SC-EHE

Accessories:

Brand: RP-Technik GmbH
