
Surveillance: 
With integrated monitoring module for operating on a Wireless Professional central monitoring system.
· Charge monitoring indicator on the luminaire
· Manual or automatic function test (free choice of test start time in the WirelessControl software)
· Manual or automatic continuous function test can be activated via the length of the luminaire’s measurement operation (free choice of test start times in the WirelessControl software)
· Automatic charge monitoring
· Deep discharge protection with restart inhibit
Matériau: PCABS,Polycarbonate
Couleur: RAL 9003
Dimensions: 73 mm x 339 mm x 71 mm

Type de montage: Deckenaufbau
Classe de protection: 2
Indice de protection (IP): IP 65
Degré de résistance aux chocs IK: IK 8
Température permise en mode contenu: 0 °C à 40 °C °C
Température permise en mode veille: 0 °C à 40 °C °C
Pictogramme: Nein

Puissance en mode continu: 5,7 W W
Puissance en mode veille: 0,8 W W
Flux lumineux en mode de secours: 520 lm lm

Tension d'entrée AC: 230 V V
Section de raccordement: 2.5 mm² mm

Batterie: LFPN3233.01-SET

Numéro d'article: PXDL423WL

Accessoires:
Numéro d'article: PXD-AW, 

Marque: RP-Technik GmbH
