The spotlight lens ensures an even distribution of light in all directions. Suited to ceiling heights well in excess of 4 metres, such as in a production site. Can also be used for open areas in hotels (operation time emergency of 8 hours). 
For optimum light distribution, it can be inserted into the respective luminaire directly at the mounting location using the quick-mounting system, depending on the application. This simplifies mounting and improves flexibility when installing.

Brand: RP-Technik GmbH
