Monitoring:

SC

Version with automatic test system in accordance with DIN EN 62034 type S including SelfControl test button:

* Test results with fault analysis (illuminant, charge and battery circuit) and status displays (operation, function test, continuous function test) using 3 colour LEDs
* Automatic function test (weekly)
* Automatic continuous function test (every 12 months)
* Automatic charge monitoring
* Deep discharge protection with restart inhibit
* Idling and short-circuit shutdown of inverter

Material: PCABS / PMMA

Color: RAL 9003

Dimensions: 101 mm x 1.277 mm x 108 mm

Mounting method: Universal

Protection class: 2

Protection rating (IP): 65

Allowed temperature DS: -5 to 35 °C

Allowed temperature BS: -5 to 40 °C

Pictogram: No

~lbl-lv-LeistungDauerbetrieb: 20,0 W

~lbl-lv-LeistungBereitschaftsbetrieb: 2,0 W

~lbl-lv-LichtstromNotbetrieb: 300 lm

Bridging time (h): 3 h

~lbl-lv-EingangsspannungAC: 230 V

~lbl-lv-Anschlussquerschnitt: 1.5 mm

Battery: MWB904,

Article number: 1LF12003SC-NW

Accessories:

Fabrikat: RP-Technik GmbH