Zinc die-cast disc luminaire according to DIN EN60598-1, DIN EN 60598-2-22 and DIN EN 1838.

German Design Award 2018-winning zinc die-cast LED disc luminaire for wall mounting.

Sober and clear design language of all A-Series luminaire versions for integration into any type of building. The modular practical design of the A-series promises the simplest installation for all variants. The design is perfectly matched for any type of mounting.

Features:
- Mechanically robust and corrosion-resistant
- Powder-coated surface
- Precise edges and straight lines
- No weld seams and bending edges
- Fixing of the pictogram solvent-free
- Panel with polished edges and continuous, invisible pictogram holder
- Mounting housing identical for all A-series variants.

Suitable for continuous or stand-by operation. Planning reliability due to tool-free, variable use of pictograms on site. Pictograms according to DIN EN ISO 7010 and DIN ISO 3864 (left, right, bottom, top) included as standard.

Material: Zinc die-cast

Color: Edelstahl gebürstet

Dimensions: 50 mm x 236 mm x 151 mm

Mounting method: Wand

Protection class: 2

Protection rating (IP): 40

Impact restistence rate IK: ≥ 3

Allowed temperature DS: -25 to 40 °C

Allowed temperature BS: -25 to 40 °C

Viewing distance: 22 m

Pictogram: Set

Power maintained mode: 2,4 W

Power non-maintained mode: 0 W

Bridging time (h): CPS

Input voltage AC: 230 V

Connection terminals: 1.5 mm

Battery:

Article number: AMW009-E

Accessories:

Article number: BALLPLX-AM, Ball protection 330x250x77mm incl. fastening

Article number: AM-X-APA, Surface mounting adapter for lateral cable feed

Brand: RP-Technik