Electrical data:

Input Voltage AC: AC 220-240V / 50-60Hz

Rated power: 8 W

Photometrical data:

Rated luminous flux: 740 lm

Colour temperature: 2200-6900 K

Light source: LED

Acceptance tests:

Protection class: II

Ingress protection (IP) rating: IP 20

Energy efficiency class: A+

Physical data:

Length (L): 115 mm

Width (B): 60 mm

Fabrikat: ROPAG GmbH