LED recessed luminaire, frame panel, EDGE series, for 625 mm ceiling module. Flat shape. Aluminium frame, white, powder-coated. Diffuser made from plastic (PMMA), opal, non-yellowing. Power supply, can be switched or dimmed (DALI/TRIAC dimmer), external. Version with CASAMBI® Bluetooth control, RGBW and tunable white available.

Electrical data:

Input Voltage AC: AC 220-240V / 50-60Hz

System power: 38 W

Photometrical data:

Rated luminous flux: 2.600 lm

Colour temperature: 4000 K

UGR: 16.6

Light source: LED

Acceptance tests:

Protection class: II

Ingress protection (IP) rating: IP 20

Energy efficiency class: A

Physical data:

Length (L): 615 mm

Width (B): 615 mm

Height (H): 15 mm

Fabrikat: ROPAG GmbH