LED safety light in accordance to DIN EN 60598-1, DIN EN 60598-2-22 and DIN EN 1838.  
  
Compact emergency lighting insert with an ovally illuminating ERT LED luminaire for the ideal light distribution on emergency escape routes. With its clear housing material, the luminaire blends in perfectly with its surroundings.   
Suitable for ceiling mounting or for installation on T5/T8 illuminants. Conventional mounting supplies like clips etc. are included in the scope of delivery. Optionally available with magnetic panel. Add-on for presenting lights without interfering with internal wiring.

Material: Plastic

Color: Opal

Dimensions: 24 mm x 50 mm x 12 mm

Material: Plastic

Color: RAL 9003

Dimensions: 36 mm x 58 mm x 250 mm

Mounting method: Deckeneinbau

Protection class: 2

Protection rating (IP): 20

Impact restistence rate IK: ≥ 3

Allowed temperature DS: -5 to 40 °C

Allowed temperature BS: -5 to 40 °C

Pictogram: No

Power maintained mode: 1,8 W

Power non-maintained mode: 0,35 W

Luminous Flux Emergency Operation: 140 lm

Bridging time (h): 8 h

Input voltage AC: 230 V

Connection terminals: 2.5 mm

Battery: NIMH9620Q, 9,6V/2.0Ah NiMH

Article number: DOE028

Accessories:

Brand: RP-Technik