LED safety luminaire according to DIN EN 60598-1, DIN EN 60598-2-22 and DIN EN 1838.   
  
LED safety luminaire for damp rooms or outdoor areas for recessed ceiling mounting made of aluminium. Two-part construction for easy sealing of the ceiling. The luminaire insert is placed in the mounting ring without tools.   
Optimum light distribution and illumination of escape and rescue routes is achieved by using powerful LED ERT technology. The light source is replaceable.

Material: Zinc die-cast

Color: RAL 9003

Dimensions: x x 110 mm

Diameter: 80 mm

Mounting method: Deckeneinbau

Protection class: 2

Protection rating (IP): 65

Impact restistence rate IK: ≥ 3

Allowed temperature DS: -5 to 40 °C

Allowed temperature BS: -5 to 40 °C

Pictogram: No

Power maintained mode: 3,5 W

Power non-maintained mode: 0,35 W

Luminous Flux Emergency Operation: 220 lm

Bridging time (h): 3 h

Input voltage AC: 230 V

Connection terminals: 2.5 mm

Battery: NIMHHT4820Q, 4,8V/2,0Ah NiMH

Article number: FGL-OUT-WEISS-023

Accessories:

Brand: RP-Technik