LED floodlight, SALO series. Housing made from die-cast aluminium for outdoor use, grey, powder-coated. Cover made from toughened glass. Operating unit installed (can be switched). DC compatible.

Electrical data:

Input Voltage AC: AC 220-240V / 50-60Hz

System power: 11 W

DC Ready: Yes

Photometrical data:

Rated luminous flux: 700 lm

Colour temperature: 4200 K

Light source: LED

Acceptance tests:

Protection class: I

Ingress protection (IP) rating: IP 65

Energy efficiency class: A

Impact resistance: IK 07

Physical data:

Length (L): 115 mm

Width (B): 86 mm

Height (H): 88 mm

Fabrikat: ROPAG GmbH