LED floodlight, SALO series. Housing made from die-cast aluminium for outdoor use, grey, powder-coated. Cover made from toughened glass. Operating unit installed (can be switched). DC compatible.

Electrical data:

Input Voltage AC: AC 220-240V / 50-60Hz

System power: 55 W

DC Ready: Yes

Rated power: 50 W

Photometrical data:

Rated luminous flux: 4.200 lm

Colour temperature: 4200 K

Light source: LED

Acceptance tests:

Protection class: I

Ingress protection (IP) rating: IP 65

Energy efficiency class: A

Impact resistance: IK 04

Physical data:

Length (L): 285 mm

Width (B): 235 mm

Height (H): 150 mm

Separable every: mm

Fabrikat: ROPAG GmbH