LED floodlight, FLOOD LIGHT series. IP66. Housing made from die-cast aluminium for outdoor use, black, powder-coated. Safety glass cover and interchangeable PC lenses, non-yellowing, for symmetric and asymmetric light distribution. Operating unit installed (can be switched). With diaphragm valve to prevent condensation.

Electrical data:

Input Voltage AC: AC 220-240V / 50-60Hz

System power: 81 W

Photometrical data:

Rated luminous flux: 13.100 lm

Colour temperature: 4500 K

UGR: 21.7

Light source: LED

Acceptance tests:

Protection class: II

Ingress protection (IP) rating: IP 66

Energy efficiency class: A++

Impact resistance: IK 08

Physical data:

Length (L): 357 mm

Width (B): 447 mm

Height (H): 61 mm

Fabrikat: ROPAG GmbH