Material: Zinc die-cast

Color: RAL 7035

Dimensions: 225 mm x 126 mm x 185 mm

Mounting method: Wand

Protection class: 1

Protection rating (IP): 65

Impact restistence rate IK: 7

Allowed temperature DS: -25 to 35 °C

Allowed temperature BS: -25 to 40 °C

Pictogram: No

Power maintained mode: 32,8 W

Power non-maintained mode: 0 W

Luminous Flux Emergency Operation: 2500 lm

Bridging time (h): ZBA

Input voltage AC: 230 V

Battery:

Article number: FL33NW

Accessories:

Brand: RP-Technik