LED escape sign luminaire according to DIN EN 60598-1, DIN EN 60598-2-22, DIN EN 7010 and DIN EN 1838.

The LED frame luminaire is suitable for wall or ceiling mounting. In addition to its linear design, it convinces with a homogeneous illumination of the pictogram. Optionally, the luminaire can be installed in the ceiling with a recessed frame.

Suitable for continuous or stand-by operation. Planning reliability thanks to tool-free, variable use of the pictograms on site. Pictograms according to DIN EN ISO 7010 and DIN ISO 3864 (left, right, bottom, top) included as standard.

Material: Polycarbonate

Color: RAL 9003

Dimensions: 45 mm x 265 mm x 208 mm

Mounting method: Universal

Protection class: 2

Protection rating (IP): 40

Impact restistence rate IK: ≥ 3

Allowed temperature DS: -25 to 40 °C

Allowed temperature BS: -25 to 40 °C

Viewing distance: 24 m

Pictogram: Set

Power maintained mode: 1,2 W

Power non-maintained mode: 0 W

Luminous Flux Emergency Operation: 32 lm

Bridging time (h): CPS

Input voltage AC: 230 V

Connection terminals: 1.5 mm

Battery:

Article number: GMU009

Accessories:

Brand: RP-Technik