LED escape sign luminaire according to DIN EN 60598-1, DIN EN 60598-2-22, DIN EN 7010 and DIN EN 1838.  
  
The LED frame luminaire is suitable for wall or ceiling mounting. In addition to its linear design, it convinces with a homogeneous illumination of the pictogram. Optionally, the luminaire can be installed in the ceiling with a mounting frame.  
  
Suitable for continuous operation. Planning reliability thanks to tool-free, variable use of the pictograms on site. Pictograms according to DIN EN ISO 7010 and DIN ISO 3864 (left, right, bottom, top) included as standard.

Monitoring:

With integrated monitoring module with 20-digit addressing switch, for operation on a central power supply system. Automatic test system according to DIN EN 62034 type ER, in connection with a system of type MultiControl. Functions must be complied with:

* Integrated individual luminaire monitoring
* Integrated luminaire manager function
* Individual switchability in conjunction with RP ELS - central power supply system

Material: Polycarbonate

Color: RAL 9003

Dimensions: 50 mm x 330 mm x 253 mm

Mounting method: Decke

Protection class: 2

Protection rating (IP): 40

Impact restistence rate IK: ≥ 3

Allowed temperature DS: -20 to 40 °C

Allowed temperature BS: -20 to 40 °C

Viewing distance: 30 m

Pictogram: Set

Power maintained mode: 4,2 W

Power non-maintained mode: 1,1 W

Luminous Flux Emergency Operation: 120 lm

Bridging time (h): CPS

Input voltage AC: 230 V

Connection terminals: 2.5 mm

Battery:

Article number: GXD009ML

Accessories:

Article number: GXE, GX recessedframe

Article number: AWX001, Wall bracket, white

Brand: RP-Technik