LED safety luminaire for illuminating escape and rescue routes in accordance with DIN EN 60598-1, DIN EN 60598-2-22 and DIN EN 1838.  
  
Compact bar-shaped plastic emergency luminaire with clear flat bonnet, for wall or ceiling mounting. Optionally, the luminaire can be installed in the ceiling with a mounting frame.  
Optimum light distribution and illumination of escape and rescue routes is achieved thanks to the diffuser lenses incorporated in the cover.

Monitoring:

With integrated monitoring module for operating on a Wireless Professional central monitoring system.

* Charge monitoring indicator on the luminaire
* Manual or automatic function test (free choice of test start time in the WirelessControl software)
* Manual or automatic continuous function test can be activated via the length of the luminaire’s measurement operation (free choice of test start times in the WirelessControl software)
* Automatic charge monitoring
* Deep discharge protection with restart inhibit

Material: Polycarbonate

Color: RAL 9003

Dimensions: 250 mm x 34 mm x 50 mm

Mounting method: Universal

Protection class: 2

Protection rating (IP): 54

Impact restistence rate IK: ≥ 3

Allowed temperature DS: -10 to 40 °C

Allowed temperature BS: -5 to 40 °C

Pictogram: No

Power maintained mode: 3,9 W

Power non-maintained mode: 1,5 W

Luminous Flux Emergency Operation: 85 lm

Bridging time (h): 8 h

Input voltage AC: 230 V

Connection terminals: 2.5 mm

Battery: LFP3233.01, 3.2V / 3.3 Ah LiFePO4

Article number: KMB018WL

Accessories:

Article number: KME-EB, KM recessed frame with test button (SB)

Article number: BALL1, Ball protection (6W) 320x220x120mm

Article number: KMBE, concrete recessed housing

Article number: BALLPLX-KMB, Ball protection 380x150x60mm incl. fastening

Article number: LFP3233.01, LiFePO4 3,2 V / 3,3 Ah

Brand: RP-Technik