LED safety luminaire for illuminating escape and rescue routes in accordance with DIN EN 60598-1, DIN EN 60598-2-22 and DIN EN 1838.

Compact bar-shaped plastic emergency luminaire with clear flat bonnet, for wall or ceiling mounting. Optionally, the luminaire can be installed in the ceiling with a mounting frame.
Optimum light distribution and illumination of escape and rescue routes is achieved thanks to the diffuser lenses incorporated in the cover.

Material: Polycarbonate

Color: RAL 9003

Dimensions: 250 mm x 34 mm x 50 mm

Mounting method: Universal

Protection class: 3

Protection rating (IP): 54

Impact restistence rate IK: ≥ 3

Allowed temperature DS: -5 to 40 °C

Allowed temperature BS: -5 to 38 °C

Pictogram: No

Power maintained mode: 2,1 W

Power non-maintained mode: 0,4 W

Luminous Flux Emergency Operation: 220 lm

Bridging time (h): CPS

Battery:

Article number: KMB519CC

Accessories:

Article number: KME-EB, KM recessed frame with test button (SB)

Article number: BALL1, Ball protection (6W) 320x220x120mm

Article number: KMBE, concrete recessed housing

Article number: BALLPLX-KMB, Ball protection 380x150x60mm incl. fastening

Article number: KMBFH, flexible wall mounting for KM

Brand: RP-Technik