Zinc die-cast escape sign luminaire according to DIN EN 60598-1, DIN EN 60598-2-22 and DIN EN 1838  
  
Escape sign luminaire for wall mounting with sober and clear design language in a flat design for integration into any type of building.   
  
Features:  
- Mechanically robust and corrosion-resistant  
- Powder-coated surface  
- Precise edges and straight lines  
- No weld seams and bending edges  
- Fixing of the pictogram solvent-free  
  
Suitable for permanent or stand-by use Planning reliability due to tool-free, variable use of the pictograms on site. Pictograms according to DIN EN ISO 7010 and DIN ISO 3864 (left, right, top, bottom) included as standard.

Material: Zinc die-cast

Color: RAL 7016

Dimensions: 48 mm x 236 mm x 148 mm

Mounting method: Wand

Protection class: 1

Protection rating (IP): 40

Impact restistence rate IK: ≥ 3

Allowed temperature DS: -25 to 40 °C

Allowed temperature BS: -25 to 40 °C

Viewing distance: 21 m

Pictogram: Set

Power maintained mode: 2,5 W

Power non-maintained mode: 0 W

Bridging time (h): CPS

Input voltage AC: 230 V

Connection terminals: 1.5 mm

Battery:

Article number: MMW009-AZ

Accessories:

Brand: RP-Technik