General and emergency luminaire according to DIN EN 60598-1, DIN EN 60598-2-22 and DIN EN 1838

Round, attractively shaped LED general luminaire made of aluminium for wall or ceiling mounting. Emergency lighting is provided with full brightness of the built-in 26W LED light source.
Housing colour choice of anodised aluminium or white
Choice of light colour 4000 K or 3000 K

Material: Aluminium

Color: RAL 9003

Dimensions: x x 113 mm

Diameter: 395 mm

Mounting method: Universal

Protection class: 1

Protection rating (IP): 20

Impact restistence rate IK: ≥ 3

Allowed temperature DS: -20 to 30 °C

Allowed temperature BS: -20 to 40 °C

Pictogram: No

Power maintained mode: 26 W

Power non-maintained mode: 0 W

Luminous Flux Emergency Operation: 2300 lm

Bridging time (h): CPS

Input voltage AC: 230 V

Connection terminals: 1.5 mm

Battery:

Article number: QAW009

Accessories:

Brand: RP-Technik