General and emergency luminaire according to DIN EN 60598-1, DIN EN 60598-2-22 and DIN EN 1838

Square recessed LED panel with all-round frame as general luminaire with emergency lighting function. Universally applicable, e.g. in system ceilings with concealed or visible trunking.

Material: Metal

Dimensions: 620 mm x 620 mm x 10 mm

Mounting method: Deckeneinbau

Protection class: 2

Protection rating (IP): 20

Impact restistence rate IK: ≥ 3

Allowed temperature DS: 0 to 40 °C

Allowed temperature BS: 0 to 40 °C

Pictogram: No

Power maintained mode: 36 W

Power non-maintained mode: 0 W

Luminous Flux Emergency Operation: 3600 lm

Bridging time (h): CPS

Battery:

Article number: ROPA4201

Accessories:

Brand: RP-Technik