General and emergency luminaire according to DIN EN 60598-1, DIN EN 60598-2-22 and DIN EN 1838  
  
Square recessed LED panel with all-round frame as general luminaire with emergency lighting function. Universally applicable, e.g. in system ceilings with concealed or visible trunking.

Monitoring:

SC

Version with automatic test system in accordance with DIN EN 62034 type S including SelfControl test button:

* Test results with fault analysis (illuminant, charge and battery circuit) and status displays (operation, function test, continuous function test) using 3 colour LEDs
* Automatic function test (weekly)
* Automatic continuous function test (every 12 months)
* Automatic charge monitoring
* Deep discharge protection with restart inhibit
* Idling and short-circuit shutdown of inverter

Material: Metal

Dimensions: 620 mm x 620 mm x 10 mm

Mounting method: Deckeneinbau

Protection class: 2

Protection rating (IP): 20

Impact restistence rate IK: ≥ 3

Allowed temperature DS: 0 to 40 °C

Allowed temperature BS: 0 to 40 °C

Pictogram: No

Power maintained mode: 33 W

Power non-maintained mode: 2 W

Luminous Flux Emergency Operation: 660 lm

Bridging time (h): 3 h

Input voltage AC: 230 V

Connection terminals: 1.5 mm

Battery: MWB904,

Article number: ROPA4201SC

Accessories:

Brand: RP-Technik