LED track luminaires, Track series, with multi-adapter for 3-phase busbars, 230V. Housing made from die-cast aluminium, white or anthracite, powder-coated. Can be rotated 350° horizontally and swivelled 90° vertically. Interchangeable PC lenses, non-yellowing, for various beam angles (20° - 60°). Operating unit can be switched or dimmed (DALI dimmer), installed.

Acceptance tests:

Protection class: II

Ingress protection (IP) rating: IP 20

Electrical data:

Input Voltage AC: AC 220-240V / 50-60Hz

System power: 22 W

Photometrical data:

Rated luminous flux: 2.500 lm

Colour temperature: 3000 K

UGR: 24.8

Light source: LED

Physical data:

Length (L): 184 mm

Width (B): 150 mm

Height (H): 85 mm

Manufacturer: RP-Technik GmbH