LED moisture-proof luminaire, VASCA ECO series, IP66, IK08. Housing and side sections made from polycarbonate, grey. Opal diffuser made from PC, UV-resistant. Symmetric light distribution and homogeneous illumination. Feed-through wiring present. Operating unit integrated, can be switched.

Acceptance tests:

Protection class: II

Ingress protection (IP) rating: IP 66

Impact resistance: IK 08

Electrical data:

Input Voltage AC: AC 220-240V / 50-60Hz

System power: 22 W

DC Ready: No

Photometrical data:

Rated luminous flux: 2.500 lm

Colour temperature: 4000 K

UGR: 24.2

Light source: LED

Physical data:

Length (L): 1.000 mm

Width (B): 62 mm

Height (H): 64 mm

Manufacturer: RP-Technik GmbH