LED safety luminaire for wall mounting to illuminate escape and rescue routes according to DIN EN 60598-1, DIN EN 60598-2-22 and DIN EN 1838.   
  
The zinc die-cast lens is locked in place without any visible fastening from the outside. The status LED built into the lens integrates into the harmony of the housing.   
The beam pattern is optimised for corridors and escape routes and is particularly powerful thanks to modern lighting technology. The light distribution aligned parallel to the wall allows mounting distances at 1Lx from luminaire to luminaire of up to 14m.  
  
Features:  
- Mechanically robust and corrosion resistant  
- Powder-coated surface  
- Precise edges and straight lines  
- No welds or bent edges  
- Suitable for continuous or stand-by operation

Monitoring:

With integrated monitoring module for operating on a Wireless Professional central monitoring system.

* Charge monitoring indicator on the luminaire
* Manual or automatic function test (free choice of test start time in the WirelessControl software)
* Manual or automatic continuous function test can be activated via the length of the luminaire’s measurement operation (free choice of test start times in the WirelessControl software)
* Automatic charge monitoring
* Deep discharge protection with restart inhibit

Material: Zinc die casting

Color: Edelstahl gebürstet

Dimensions: 53 mm x 193 mm x 115 mm

Mounting method: Wand

Protection class: 2

Protection rating (IP): 20

Impact restistence rate IK: 4

Allowed temperature DS: -5 to 35 °C

Allowed temperature BS: -5 to 40 °C

Pictogram: No

Power maintained mode: 3,9 W

Power non-maintained mode: 0,8 W

Luminous Flux Emergency Operation: 420 lm

Bridging time (h): 1 h

Input voltage AC: 230 V

Connection terminals: 2.5 mm

Battery: LFP3212-LEO, 6.4V/1.2Ah LiFeP04

Article number: WAF421WL-E

Accessories:

Brand: RP-Technik