Acceptance tests:

Protection class: II

Ingress protection (IP) rating: IP 20

Electrical data:

Input Voltage AC: AC 220-240V / 50-60Hz

System power: 42 W

Photometrical data:

Rated luminous flux: 4.750 lm

Colour temperature: 4000 K

UGR: 18.1

Light source: LED

Physical data:

Height (H): 110 mm

Ceiling Cut-out ø: 155 mm

Diameter ø: 162 mm

Producent RP-Technik GmbH