Acceptance tests:

Protection class: II

Ingress protection (IP) rating: IP 44

Electrical data:

Input Voltage AC: AC 220-240V / 50-60Hz

System power: 37 W

Photometrical data:

Rated luminous flux: 3.400 lm

Colour temperature: 3000 K

Light source: LED

Physical data:

Height (H): 80 mm

Ceiling Cut-out ø: 160 mm

Diameter ø: 172 mm

Producent RP-Technik GmbH