LED high-bay luminaires, High Bay series, for wire or chain suspension, IP65. Die-cast aluminium housing, powder-coated. Interchangeable PC lenses, non-yellowing, for various beam angles (60°, 90°, 120°). Operating unit can be switched or dimmed (DALI dimmer). Version with CASAMBI® Bluetooth control available.

Acceptance tests:

Protection class: I

Ingress protection (IP) rating: IP 65

Impact resistance: IK 10

Electrical data:

Input Voltage AC: AC 220-240V / 50-60Hz

System power: 200 W

Photometrical data:

Rated luminous flux: 28.000 lm

Colour temperature: 4000 K

Light source: LED

Physical data:

Height (H): 233 mm

Diameter ø: 380 mm

Manufacturer: RP-Technik GmbH