Use the CO-CBUBOX as the main switch for all modules and luminaires and at the same time enjoy the positive side effect of using less power. The CBU BOX can be used to switch all modules in a fully de-energised manner so that no standby current is consumed when switched off. In storage facilities or production areas with large numbers of floodlights and modules, you can therefore benefit from huge energy savings.

Electrical data:

Input Voltage AC: AC 220-240V / 50-60Hz

Acceptance tests:

Protection class: II

Ingress protection (IP) rating: IP 65

Physical data:

Length (L): 162 mm

Width (B): 116 mm

Height (H): 76 mm

Manufacturer: RP-Technik GmbH