This module permits direct access to all key functions of the CASAMBI® lighting control, so is similar to the PWM4 module. The PWM300 can, however, supply consumers with a power consumption of up to 300 W.

Electrical data:

Output max.: 300 W

Switching output: W

Input Voltage DC: 30 V

Acceptance tests:

Protection class: III

Ingress protection (IP) rating: IP 20

Physical data:

Length (L): 100 mm

Width (B): 29 mm

Height (H): 13 mm

Manufacturer: RP-Technik GmbH